

USB DRIVER INSTALLATION
-----------------------
This .zip file contains the USB drivers. Extract this file into any folder on your computer. The EV2300 USB board should then be connected to the computer. If the driver has not already been installed, Windows will pop up a wizard to ask for the driver files. You can just browse to the folder where you put the drivers, and click on the USB Driver folder there. If you are using Windows 98, then select the TIUSBWin98 folder. For Windows 2000 or XP, select the TIUSBWin2K-XP-1 folder.

There are two drivers required for the EV2300 board, so the wizard may ask you twice. For Windows 98, you always point it to the USB Win98 folder. For Windows 2000 and XP, you may have to reboot in order for the wizard to query for the second driver. The second driver is in the TIUSBWin2K-XP-2 folder.

This can be tricky with Windows 98 because the wizard doesn't always work. As an alternative, you can use the Control Panel option to add new hardware and a wizard there will help to install the driver.

